****

**Selling Price:** $355,000 USD

**FOB:** Manchester, Connecticut, USA

**Availability:** Immediate

Plus Applicable Taxes / Subject to Prior Sale

**One (1) Used 2016 Grove GHC55, S/N: 55.5.214, 55 Ton Capacity Telescopic Boom Crawler Crane, Equipped As Shown Below:**

|  |  |
| --- | --- |
| - 30’ 10” – 99’ 9” 4-Section Sequenced Synchronized  Full Power Main Boom- 21’ 4” Offsettable Swingaway Extension- Swingaway Offsetts at 0 and 40 Degrees- 21’ 4” Fly Jib Extension - Auxiliary Boom Nose- Five Sheave Main Boom Nose- Main & Auxiliary Hoists- Drum Rotation Indicators- Operator’s Cab Tilts to 15 Degrees- Ergonomic Control Panels- Load Sensing Electric Dual Axis Control Joysticks- Radio Remote Control System - Air Conditioning for Operator’s Cab- Pole Claw Preparation with Tool Circuit- 360 Degree Continuous Swing | - Pinion Lubrication for Slewing Gear w/ Pump - Cummins QSB4.5 (Tier IV Final) Diesel Engine- 19,621 Lbs Total Counterweight- Hydraulically Extendable Undercarriage- Maintenance-Free Crawlers (59 Track Shoes)- 36” Triple-Bar Track Shoes - 2-Stage Track Motors for High Travel Speed- “Graphical RCL” Load Moment Indicator- External RCL Light Bar- Windspeed Indicator Displayed through RCL- Anti Two Block & WADS “Work Area Definition” Systems- One Rotating Beacon Light on Top of Cab- Two Additional LED Lights Mounted on Base Boom- Foldable Catwalk on Both Sides of S/S- 38.5 Ton 3-Sheave Hookblock- 5.5 Ton Headache Ball- Approximate Hours: 2,692 Hours (6/8/22) |

**2016 GROVE GHC55, S/N: 55.5.214**

55 Ton Telescopic Boom Crawler Crane